## The Project Gutenberg eBook of On the Processes for the Production of Ex Libris (Book-Plates)

This ebook is for the use of anyone anywhere in the United States and most other parts of the world at no cost and with almost no restrictions whatsoever. You may copy it, give it away or re-use it under the terms of the Project Gutenberg License included with this ebook or online at www.gutenberg.org. If you are not located in the United States, you will have to check the laws of the country where you are located before using this eBook.

Title: On the Processes for the Production of Ex Libris (Book-Plates)

Author: John Vinycomb

Release date: May 14, 2020 [eBook #62127]
Most recently updated: October 18, 2024

Language: English

Credits: Produced by deaurider, Paul Marshall and the Online
Distributed Proofreading Team at https://www.pgdp.net (This
file was produced from images generously made available
by The Internet Archive)

*** START OF THE PROJECT GUTENBERG EBOOK ON THE PROCESSES FOR THE PRODUCTION OF EX LIBRIS (BOOK-PLATES) ***

[Pg i]

# ON THE PROCESSES FOR
THE PRODUCTION OF
EX LIBRIS
(BOOK-PLATES)

By John Vinycomb, M.R.I.A.

Fellow of the Royal Society of Antiquaries of Ireland
President of the Belfast Art Society, 1891-92
Member of Council of the Ex Libris Society

Reprinted from the Journal of the Ex Libris Society
with additional illustrations.

[Pg ii]

LONDON:

A. & C. BLACK, Soho Square
1894

[Pg iii]

TO
ARTHUR VICARS, F.S.A.,
ULSTER KING OF ARMS

A VICE-PRESIDENT OF THE EX LIBRIS SOCIETY
AND AN EMINENT COLLECTOR

I RESPECTFULLY DEDICATE
THIS LITTLE BOOK.

[Pg iv]

Franklin Press.
Now at Philadelphia, U.S.A.

[Pg v]

## PREFACE.

In acceding to the author’s request that I would add a few words of introduction to these reprinted articles, I do so with pleasure, although entering a mild protest thereon, inasmuch as the writer has handled his subject so well that it leaves very little to say, except in commendation of the work to the favourable consideration of those for whom it was written.

Mr. Vinycomb has in these articles aimed to give his readers a practical dissertation upon the modes of execution, rather than upon the history and classification of styles in the production of book-plates; and in this he has certainly departed from the beaten track, and has furnished a very concise and clear account of the various processes by which our book-plates are produced and reproduced, and the numerous and ingenious methods of manipulation resorted to in their manufacture.

Some people may take exception to the word manufacture, used in this connection, as being inappropriate to a description of what may be defined as one of the modern arts. But the terms, though by no means synonymous, are at any rate akin; for doubtless the majority of book-plates are artistically designed, but for their reproduction and final manipulation the aid of science must be resorted to. [Pg vi]

Mr. Vinycomb, in his opening remarks, says: “The production of book-plates, by whatever means, is but a side branch of the art by which pictorial and decorative illustrations of every kind are executed, and copies multiplied by some of the ordinary processes of printing.” He then tells us that whereas in former times wood engraving and copper engraving were responsible for most of the book-plates existing, “the advance of modern science has, however, changed all that, and we may now possess a charming book-plate, which is neither engraved on wood or on copper, and yet may pass for either the one or the other, or have characteristics entirely its own.” It must be borne in mind, however, that many persons have a great abhorrence of processes of all kinds, and cannot be satisfied with anything short of an Ex Libris worked direct from the copper. In the highest interests of Art, they are doubtless right; but whereas it is only the rich man who can purchase the work of an old master or of a modern painter, by means of the despised process blocks these same works of art can be placed in the hands of everyone. This, however, is too wide a subject to be dealt with here; yet a glance at the pages of the Studio and other current periodicals should convince the most sceptical that the most beautiful work may be produced by these same processes. It is the same with book-plates, the artist’s handiwork being reproduced in absolute fac-simile.

Mr. Vinycomb leads us, in these pages, by easy stages, through the various developments of engraving, from the rough woodcuts which are to be found in the earliest printed books to the beautifully finished work [Pg vii] of Dürer and other masters of engraving. Then comes the engraving on metals and etching; and last we are let into the secrets of the various means adopted for the duplication of artists’ sketches by means of blocks or transfers, from which any number of copies may be taken. He has, as we have already stated, treated his subject in an eminently practical manner, so that the veriest tyro may be able to understand the methods used in the multiplication of Ex Libris; and by means of the well-selected illustrations, and the hints so freely scattered over these pages, it is an easy matter for those who have not studied the art of engraving and process-working to gain a fair knowledge of the subject.

Some of the illustrations have already appeared in connection with these articles in the Ex Libris Journal (Vol. III., pp. 151, 170; Vol. IV., pp. 17, 43, 57, 92); others are introduced here for the first time; but they are all well calculated to enhance the value of Mr. Vinycomb’s work, and to show what can be done by the various methods in use. Further, it may be safely assumed that all systematic collectors of book-plates will be glad to have in this handy and independent form an essay upon the practical side of a subject in which they have up to the present taken, perhaps, but a general or sentimental interest.

Thanks to the formation of the Ex Libris Society, the collection and preservation of book-plates has now reached something akin to a scientific position, and in large and valuable collections it has become more and more necessary to know how best to classify and arrange our acquisitions. This knowledge can therefore best be secured by studying such works as the present, by means of which the collector is [Pg viii] able to judge of the age and value of a plate, or at any rate to fix an approximate date to those (and they are many) which have no printed date to fix their identity.

This little work comes as a valuable companion to Mr. Hamilton’s recently published work on “Dated Book-plates,” in which he deals with almost all the branches of the subject of most interest or value to collectors, but has, naturally, little to say upon the practical production of Ex Libris—leaving that to an expert in the person of the writer of the present essay. For practical engravers Mr. Vinycomb has probably said too much, or not enough, or has, perhaps, only told them what they knew already; but as the majority of collectors cannot be classed in this category, it may fairly be assumed that the author has filled a gap in book-plate literature which no previous writer has attempted to supply, and that his work will be found of great value to members of the Ex Libris Society, and to collectors of book-plates in general.

W. H. K. WRIGHT,
Editor Ex Libris Journal.

[Pg ix]

## CONTENTS.

| Page
Preface | v.
Introduction | 1
Wood Engraving | 9
Engraving on Copper and Steel | 27
Lithography | 58
Chromo-Lithography | 65
Photo-Lithography | 65
Drawing for Photo-Litho. and Process Work | 67
Process Blocks—Line Work | 69
” Half-tone Blocks | 83
Hints to Collectors of Ex Libris | 91
“Au Revoir” | 95

[Pg x]

EX LIBRIS ILLUSTRATIONS.

R. S. Mansergh—Armorial, printed in tinctures |
by Chromo-Lithography | Frontispiece
Modern Engraved Plates— | Facing Page
R. Day, F.S.A., engraved by C. W. Sherborn, |
printed from the copper-plate | 27
R. Day, F.S.A.—Vesica Armorial |  | printed by |  | 1
lithography
R. S. Mansergh—Armorial | ” | 42
Edward Cox—Circular Armorial | ” | 45
W. H. K. Wright, F.R.HIST.SOC. |  | ” |
—Library Interior | 47
R. Day, F.S.A.—Pictorial, Etching | ” | 48
R. J. Welland, Bishop of Down and Connor |  | ” |
and Dromore | 52
J. F. Wilson—Circular Armorial | ” | 54
J. Neville Cross—Circular Seal Armorial | ” | 56

Lithographed and Photo-Lithographed Examples—

Joseph McChesney—Pictorial | 58
Robert Day, F.S.A.—Library Interior | 60
Fredk. Arthur Beale—Armorial | 62
Wood Institute, Rugby—Decorative | 64
Robert Day, F.S.A.—Ogham, Landscape, etc. | 66
Free Public Library, Belfast—Decorative Arm. | 70
Rev. J. H. Bibby—Library Interior | 72
Robert Cochrane, C.E., F.R.I.B.A., F.S.A., etc.—Armorial | 80 [Pg xi]

EX LIBRIS ILLUSTRATIONS IN THE TEXT,

Reproduced by Process Blocks.

| Page
J. H. Fryer—Etching, Landscape, by Lambert, Newcastle | 1
Brandenburg or Buxheim plate—Early wood engraving | 8
Hans Igler plate—Early wood engraving (double-page) | 14
Kress of Kressenstein, by Albert Dürer | 17
Wm. Taylor, by Bewick—Wood engraving | 19
(No name)”” | 21
Kress of Kressenstein, by Hans Troschel, engraved on copper | 28
Samuel Pepys—Portrait plate by R. White, engraved on copper | 31
Henʸ. Jaˢ. Pye—Chippendale plate by Playner | 33
—— Barrow—Armorial Book-pile, by Lightboune, engraved on copper | 36
William Cowper—Decorative Armorial, engraved on copper | 39
Ellis Gamble—Decorative Armorial, by William Hogarth, engraved on copper | 40
William Hogarth—Decorative Monogram plate, engraved on copper | 41
Edw. Loveden Loveden—Engraved on copper | 44
H. Stamford—Pictorial, etching on copper | 49
James Neild |  | Two Pictorial Etchings by Bewick | 51
—— Spence
Joseph Pollard |  | ”” | 53
Chas. Fenwick
Charles Bragge—Urn Armorial, etching | 57
Arthur Vicars, F.S.A., Ulster King of Arms—Pen and ink, by Rev. W. FitzGerald | 68 [Pg xii]
Francis Joseph Bigger, M.R.I.A.—(Old Belfast) Pen and ink | 70
Robert Day, F.S.A.—Armorial Masonic | 72
Walter Besant, M.A.—Library Interior | 74
Francis Joseph Bigger—Armorial | 76
George Rollo—Smithy Interior | 78
F. D. Ward, J.P., M.R.I.A., CH.L.H.—Armorial | 80
I. M. F. H. Stone, M.A., F.L.S., F.C.S.—Armorial | 82
Arthur Acton—Emblematic | 84
Belfast Art Society, 3 sizes—Emblematic | 86
Dublin Naturalists’ Field Club | 88
Masonic Province of Down—Armorial Masonic | 90
John Vinycomb, M.R.I.A.—Armorial | 96
Fine Half-tone Process Blocks— | Facing Page
Antiquarian subject, reproduced from Mono-tint Drawing | 83
Virgin and Child, reproduced by Aquatint Engraving | 89
George G. Ward, reproduced from Design in Colours for Stained Glass | 93
Vinicombe Bey, reproduced from Soft-ground Etching | 94

ILLUSTRATIVE CUTS IN TEXT.
Franklin Press, now at Philadelphia | iv.
Caxton’s “Printer’s Mark” | 9
Form-Schneider at Work | 13
Engraver’s Knife, from Papillon’s Treatise, 1766 | 15
Press of Ascensius | 16
Engraver’s Tools | 24
Mode of Engraving | 25
Copper-plate Printing Press | 46
Lithographic Printing Press | 58

[Pg xiii]

[Pg xiv]

Transfer, direct from Engraved plate to stone.

Etching on copper by Lambert, Newcastle, reproduced by process block.

From the collection of W. H. K. Wright.

[Pg 1]

## ON THE PROCESSES FOR THE
PRODUCTION OF EX LIBRIS.

By John Vinycomb, M.R.I.A.

### Introductory.

The production of book-plates, by whatever means, is but a side branch of the Art by which pictorial and decorative illustrations of every kind are [Pg 2] executed, and copies multiplied by some of the ordinary processes of printing. Without, at this stage, going minutely into the history of pictorial illustration and printing, it may be briefly stated that in times past, the only available modes of reproduction were either by engraved wood blocks with the lines in relief to print with letterpress, or by engraved copper-plates having the lines cut into the polished surface of the metal and printed by the copper-plate press (the modus operandi in each method will be explained later on).

The processes for the production of Ex Libris—as it is now the fashion to term these dainty little works of art we so delight to collect and preserve—are to-day so numerous and so varied in their style and character of work as to be wholly dissimilar, yet in very many instances we find the results to be so nearly alike that only a practical expert can, with any degree of certainty, state how and by what means they have been executed. It is not therefore surprising that [Pg 3] the collector—that picker-up of unconsidered trifles—however deeply versed he may be in the literature of the subject, for want of some technical knowledge should sometimes be mystified and unable to declare how a particular specimen has been produced. In the older examples there is little or no difficulty in distinguishing the difference between a woodcut and a print from a copper-plate; to one or the other of these two methods it must of necessity belong. The advance of modern science has, however, changed all that, and we may now possess a charming book-plate, which is neither engraved on wood nor on copper, and yet may pass for either the one or the other, or have characteristics entirely its own.

Some account of these two older methods and their later developments, as well as a sketch of some of the modern processes arising out of the invention of lithography and photography, will be of interest to collectors of Ex Libris; particularly the process blocks so much in [Pg 4] vogue at the present time for high-class book illustrations, magazines, the illustrated weeklies, etc., by means of which the artist’s drawing, through a happy union of these later arts and chemical science, may be translated into a printing surface of metal or other material for giving off impressions by the type press, the copper-plate press, by lithography, or by one of the photo-mechanical processes, such as calotype, etc. By reference to representative examples, it is hoped to enable the collector to form a pretty accurate idea of the mode of execution of similar works.

Whatever merit of originality or of fancy the earlier examples may possess, it is interesting to observe how largely book-plates partake of the prevailing style or fashion of the times. By this test alone, collectors are led almost to a certainty to fix an approximate date when they were designed and engraved. Again, how clearly the character [Pg 5] of the artist appears upon the face of each example, whether he was a “base mechanick” at his trade, or a true artist, who lent his thought and skilful hand to embellish the library of his friend or client. The artist himself, in old times, generally a versatile many-sided man, adapted himself to his work and wrought out his ideas con amore in whatever direction he might be called upon, whether it was to paint some great picture, to draw and perhaps engrave on wood or copper some of his immortal conceptions, or it may be only a simple book-plate for his friend and patron. Such a man was Albrecht Dürer. A book-plate by him, cut on wood, for his friend, Bilibaldi Pirckheimer, forms the frontispiece to the Hon. Leicester Warren’s book on “The Study of Book-plates.” Men like Michael Angelo, who could vary his occupation to every phase of Art, now as an architect, conceiving and carrying out the erection of the great Church of St. Peter’s at Rome, painting the [Pg 6] grandest and most sublime pictures, and in sculpture without a rival, but who could also bring his lofty mind to the consideration of works of less importance. To him, to Hans Holbein, and others of highest rank as artists, we are indebted for the immense advancement of the fine arts at this period, which, starting with the Renaissance of Literature and Art in the 15th and 16th centuries, gradually dispersed the darkness of the middle ages. Drawing and engraving on wood were brought to a high degree of perfection, and a race of artists was educated, who devoted themselves exclusively to illustrating books which the recently invented art of printing had called into requisition.

Wood engraving, as an adjunct to printed books, was the earliest form in which good art became popularised: book illustration by engraved copper-plates was a later development, though the art was not unknown: at a later period, copper-plate illustrations almost entirely superseded wood for the purpose. [Pg 7]

One who has carefully studied the illustrations in early-printed books—from printer’s mark on title-page to colophon—cannot fail to be struck with the manly and vigorous style of drawing in the cuts, shewing a real grasp of the subject and mastery of detail, and while we may be amused at the quaint conceits, and somewhat crude lines, we cannot but be charmed with the natural simplicity of the drawing, though lacking almost entirely in local colour. In the infancy of the art of engraving on wood, it necessarily followed that there should be some want of refinement in the execution. The engraver on wood was born very young, and had to grope his way by tedious practice to acquire skill and knowledge for his work. The artist, on the contrary, like Minerva, came into being fully equipped, or, to be literal, he already existed; with mature experience he adapted his skill to the requirements of the new art, the first and most important being that, [Pg 8] as the tools of the engraver and the wood he used were unfitted for small details, the lines to be drawn by the artist on the wood must necessarily be few and well chosen.

The Brandenburg, or Buxheim plate, circa 1480.

[The oldest Ex Libris actually connected with a printed book.
See Ex Libris Journal, Vol. II., p. 71.]

Fig. 4.—DEVICE COMMONLY ATTRIBUTED TO CAXTON.

Caxton’s Mark.

[Pg 9]

## WOOD ENGRAVING.

Beyond giving some idea of what wood engraving is and how it is produced, it is not intended to do more than refer to the early history of the art—a subject on which bulky volumes have been written—or to enter minutely into the details and modes of execution of modern work. To those who desire further information, special works on the subject may be consulted.[1]

[Pg 10]

### WOOD ENGRAVING AND COPPER-PLATE
ENGRAVING—THE DIFFERENCE.

Copper-plate engraving, which almost entirely superseded wood in the seventeenth and eighteenth centuries, differs in principle from wood engraving in this—that a woodcut has the lines of the design standing up in relief, the wood between the lines incised or cut away, so that when the surface is inked the lines so charged will give off an impression upon paper by rubbing the back, or by the use of the type press. In the copper-plate the lines are cut into the polished surface of the metal, which, when smeared over with printing ink, and the surface wiped clean, leaves the incised lines filled with ink; an impression is taken by the use of a press specially adapted to the purpose.

It will be seen that surface printing is the necessity and characteristic of wood engraving. Simple and crude in its beginnings, [Pg 11] owing chiefly to the imperfect mechanical means of cutting the wood in sufficiently fine or exact lines; it was employed first in the production of playing cards, the outlines of which were formed by impressions from wood blocks, and the colouring filled in by hand or stencil. In Europe the earliest application of the art to pictorial illustration took place in Germany about the close of the fourteenth or beginning of the fifteenth century. The oldest woodcut with a date known is of 1423. It represents St. Christopher carrying our Saviour on his shoulders across a river. Other specimens, though undated, from their greater rudeness, have been held to have superior claims to antiquity. With the invention of printing the art soon made rapid strides, and on the introduction of moveable types to print in conjunction with engraved blocks, a new impetus was given to the production of engraved wood blocks. In the early part of the sixteenth century, several artists of celebrity were either designers on wood or [Pg 12] engravers. Books at this period were profusely illustrated. Among the most distinguished in this line was Albert Dürer, whose productions as a painter and an engraver on copper and wood are so numerous that he could not possibly have engraved a tithe of the wood engravings attributed to him; probably he only put the design on the blocks, leaving them to others to execute.

The art was chiefly practised in Germany, where it was patronised by the Emperor Maximilian, for whom Burgmair produced the great work, “The Triumphs of Maximilian.” The next great name in the annals of wood engraving is that of Hans Holbein, whose “Dance of Death” was printed in Lyons in 1538.

In England Caxton brought out his “Game and Playe of Chesse” in 1476, with cuts. There are woodcuts also in the “Golden Legend,” 1483; “Fables of Æsop,” 1484; Chaucer’s “Canterbury Tales,” and other books of [Pg 13] his printing—all scarce and poor in execution, but noticeable in the history of Art. From 1545 to 1580 wood engraving continued to be much used for illustrating books in England, chiefly by John Daye. From this period there is little to be recorded of essential importance till the appearance of Bewick, to whom the revival of wood engraving is chiefly to be attributed.

Form-schneider.

[Pg 14]

### EARLY METHOD OF ENGRAVING ON THE SIDE
OF THE WOOD WITH KNIVES.

In early days of wood engraving a close-grained slab of wood of a suitable thickness to print with type was used for the purpose by the engraver—cut the long way of the tree, and not upon the end or section of the wood as in modern work; and the cutting was necessarily executed with the knife. The quaint and rude cut on the accompanying double page is a fair example of the earliest species of woodcut, and is the most ancient Ex Libris known.

Regarding the knife as a cutting instrument, Mr. W. J. Linton, in his “Manual of Wood Engraving,” p. 28, says: “As far as I have been able to ascertain, with the one possible exception of the cuts to Croxall’s Fables, 1722, all engravings on wood from the earliest time to the time of Bewick were done with the knife instead of gravers.”

Rude Early Woodcut. (Actual size.)

The most ancient Ex Libris known. It is Jean Knabensberg, called Igler, chaplain to the family of Schönstett. It represents a hedgehog with a flower in its mouth. In the banderole we read, “Hanns Igler das dich ein Igel Kuss.” Its approximate date is 1450. Herr Ludwig Rosenthal, antiquariat, Munich, has a copy of this rare plate in his possession, which he values at 600 marks. See Warnecke’s “Die deutschen Bücherzeichen” (Ex Libris), 1890.

[Pg 15]

From Papillon’s Treatise, 1766.

We can to some extent realise the difficulties the early wood engravers laboured under in this respect in producing fine work, but when we examine the later works of the German engravers, and observe the gradual improvement from crudeness to really excellent work, we are amazed that with such disabilities such splendid results were attainable by the knife. The Form-schneider, as the engraver of block pictures was termed, increased in skill and dexterity in deftly cutting the design exactly as it was drawn on the wood, and with exceeding truthfulness; using a finer grained and harder wood and tools more perfectly adapted for the work, so would the art [Pg 16] advance by leaps and bounds, until in the time of Dürer and Holbein it had reached its high-water mark of excellence. Boxwood was then, as now, in use, but for delicate work only, and cut plank-wise. For larger work softer woods were good enough: pear and apple woods, privet, sycamore, and any white wood upon which a drawing could be [Pg 17] seen—everything being drawn line for line on the plank; the engraver’s business simply to cut away the white spaces between the lines, cutting, as before said, with knives in the smaller spaces, and with chisels and gouges clearing away the larger to a sufficient depth to escape the ink in printing.

Press of Ascensius.

Small Dürer Woodcut, of the Nuremberg family of Kress of Kressenstein.

[Pg 18] At the present day, in the skilfully drawn and engraved block books of the Japanese, the illustrations will be found to be drawn with the brush upon the side of the wood, and cut with a knife; but we are not now astonished at anything done by this wonderful people, who have knocked the wind out of us in so many forms of art.

### MODERN WOOD ENGRAVING.

To understand the scope and practice of wood engraving, it will be necessary to glance through the illustrated publications of a few years ago, before process blocks had to so large extent superseded the work of the graver. The immense popularity the art has obtained in this country owing to the establishment of the Illustrated London News, Graphic, Art Journal, Magazine of Art, and similar publications, not to speak of book illustrations, has been remarkable. The excellence of the work and the infinite variety of style introduced by the best [Pg 19] artists and engravers show it to be capable of representing every artistic quality supposed to be peculiar to copper and steel engraving; [Pg 20] other qualities it has, such as power and force in the darker portions, and the use of white-line work on tint, or solid ground—effects obtained with extreme difficulty upon the metal plate.

Ex Libris engraved on wood by Bewick, reproduced by process block.

Wood engraving for pictorial work may be divided into two kinds:—

I.—Black-Line or Fac-simile Work.—The drawing on wood is engraved exactly as it is drawn, line for line. All examples up to the time of Bewick, and a great many since, are of this kind. As illustrating the best qualities of this style of wood engraving, no more apt examples could be named than the cartoons and drawings in Punch by Tenniel, Doyle, Leech, and others, before the introduction of photo-etched process blocks. (Bewick himself, an artist as well as an engraver, made a departure from the old crude manner of wood engraving by introducing a new style of work, imitating more truly the local colour and the [Pg 21] textures of nature: drawing the subject of the design on wood in pencil and afterwards tinting in the masses of shade and local colour with washes of china ink; and with the graver giving all the characteristic markings and minuter details by white lines upon the dark ground. In his Natural History Cuts he imitated in the most marvellous manner the textures of trees, grass, and natural scenery, [Pg 22] the plumage of birds, the shaggy or smooth coats of animals, etc. A number of Ex Libris executed by him on wood have the same characteristic handling). The two wood engravings by Bewick are reproduced by process blocks. Though inferior to many of his Natural History Cuts, they fairly show the style and character of his handiwork—the careful execution of details and the use of white-line work upon solid black ground.

(From the Collection of W. H. K. Wright, Esq.).

Wood Engraving by Bewick.

II.—Tinted Work.—In this mode the subject is drawn in TINTS OR WASHES, and partly with the pencil. To be successful in work of this kind, to interpret the artist’s ideas truly, the engraver must himself be an artist of considerable ability, as he has to adapt the lines to the work, and in this lies rare judgment and discretion, as not only the direction of the line most conducive to develop the form, but the width and thickness of the lines and spaces must be accurately judged; the various qualities of surfaces must likewise be suggested by the engraved lines. [Pg 23]

### MATERIALS AND MODE OF PROCEEDING.

The wood used by engravers is boxwood, on account of its close grain and firm texture; it is principally imported from Turkey, cut transversely or across the grain (so that the engraving is done upon the end way of the wood). It is made seven-eighths of an inch in thickness (type height). It takes a beautifully smooth surface, and cuts under the graver with the utmost clearness and fineness. The polished surface of the wood being unsuitable for drawing on, a slight “tooth” is given to it by a little water-colour white rubbed over the face of the block with the ball of the thumb until nearly dry, when it presents a pleasant surface for the pencil.

The drawing or design having been sketched out and perfected on paper, it is then traced the reverse way upon the wood block, and the drawing then worked out, either in black-line fac-simile or in tints, as may be intended. The black lead pencil, of sufficient hardness of lead [Pg 24] to stand the pressure upon the solid surface, is the favourite instrument for drawing. For tinting, either the pencil or the brush with washes of china ink can be used.

The tools used are gravers, tint-tools, and scoopers, or cutting out tools—in all about a dozen different sizes; the several kinds are here indicated. With the gravers the outline and all the details are cut; the tints, by which the proper tones or light and shade are obtained, can best be rendered with tint-tools of various widths of [Pg 25] cut. The parts not required to be printed are hollowed out with scoopers. It will be understood that all the blanks or white parts of an engraving have been cut away in the block.

Mode of Engraving on Wood.

There are several et ceteras also required by the engraver, as, an oil-stone to sharpen his gravers; an eye-glass, when engraving very [Pg 26] fine work; a small circular sand-bag, on which the block is held while being engraved; an instrument called a burnisher, with which to take proofs. A glass globe filled with water, to concentrate the light from lamp or gas jet upon the block, is used at night.

The engraving being completed, the surface of the block is inked very lightly with printing ink, and a piece of India paper, or any fine paper of similar quality, being laid upon it, an impression is taken by rubbing the paper with the burnisher until it is fully printed. From this proof the engraver can judge whether any alterations are required and what improvements can be effected.

The revival of wood engraving by Bewick and others, and the high state of perfection to which it had been brought by his immediate successors, to a very great extent superseded copper-plate engraving for book illustrations, though for Ex Libris, copper-plate held, and still holds its place as the chief and deservedly favourite style.

Crest Ex Libris of R. Day, F.S.A., Cork.

Engraved by C. W. Sherborn, and printed direct from the Copper-Plate.

[Pg 27]

## ENGRAVING ON COPPER
AND STEEL.

Where be the equal now of those glorious editions of the poets, the “Annuals,” “Keepsakes,” “Books of Beauty,” and other delightful volumes that still charm the eyes and glad the hearts of those who have the taste and the wit to possess them? As works of the highest art quality, they have never since been equalled for beauty of work, with their engraved titles, frontispieces, and illustrations in the text, drawn by Stothard, Turner, Creswick, Stanfield, Harding, and a host of the first names in British Art, and engraved in the rarest and most exquisite manner by men equally eminent in their line. “Woodcuts,” however, cut them out for the time, owing to the excellence to which the art had attained, and the greater rapidity and cheapness in printing. [Pg 28]

Kress Book-plate.
(See Ex Libris Journal, Vol. IV., p. 9.)

Engraved on Copper by Hans Troschel, 1699.
Reproduced by process block.

[Pg 29] In all the changes and inventions in the modes of art reproduction the engraved plate has steadily held its own as the most finished and perfect. For Ex Libris it is particularly suitable; it is par excellence THE STYLE for the attainment of the highest art quality.

The Art Journal, supported by one or two similar publications, has heroically endeavoured to maintain the traditions of the best period of the Art in its steel-plate illustrations, but, except for pictures of this kind, and of larger size for framing, illustrations on steel and copper for books may be said to be practically extinct.

Time, however, has its revenges: wood engraving, in its turn, is being rapidly displaced by “process blocks” (of which more anon), and now, if we take up any recent illustrated book or journal, we find the bulk [Pg 30] of the pictures and designs not wood engravings but process blocks.

In every good collection of Ex Libris the majority of examples will be found to be printed from engraved plates, very few relatively being from wood blocks. The reason is not far to seek. The wood engraving as practised in England previous to the opening of the present century was poor in execution, and did not lend itself sufficiently to working out minute details with the same ease and readiness with which they can be executed on copper.

Pure Line Engraving by Robert White,
from a Painting by Sir Godfrey Kneller.

Reproduced by process block.

That it was the favourite mode of producing these dainty little works is evident also from the fact that copper-plate pictures for book illustrations of every kind had almost entirely superseded wood engraving, which had indeed fallen completely into disfavour. Until the beginning of the present century, when Bewick and others had elevated it into a fine art, wood engraving was in an exceedingly rude condition, [Pg 31]
[Pg 32] and little fitted for small works. Copper-plate engraving, on the contrary, had for several centuries flourished successfully; every goldsmith was able to “chase” and engrave the decorative and heraldic work upon silver plate and goldsmiths’ work, or upon metal of any kind, in relief, or intaglio, as in medals, coins, etc. That this is no mere assumption we know from historical evidence, as well as from a careful comparison of the “handling,” or the manner of cutting the lines upon silver work, which is identical with the style of cutting the lines in so very many engraved book-plates of the last and early part of the present century. Whatever may be thought of the vagaries of the accessories in the Jacobean, Chippendale, and other kindred styles—which are essentially silver engraving patterns—much of this class of work shows at least a true heraldic spirit in the treatment of the charges. [Pg 33]

A Chippendale pattern. Silver Engraver’s style of work,

reproduced by process block.

[Pg 34] Benvenuto Cellini, whose works now bring fabulous prices in goldsmith work, was an expert engraver as well, as were probably most of the workers in the precious metals of his time. Hogarth, in the earlier part of his career, did much in the way of engraving arms, crests, etc., for the silversmiths; so did Bewick, who worked on wood and on metal indifferently. The writer has done a fair share of similar work in his younger days; and to his knowledge it was the custom in many establishments for the engravers to do both, as the exigencies of business required, though the tendency when work was plentiful was to specialise, each man doing that part for which he seemed to have an aptitude. This refers particularly to graver work; the pictorial engraver executing his work principally by means of the etching process, and only finishing up with the graver.

No doubt a life-long practice in one particular class of work of this [Pg 35] kind is calculated to engender a stiff and formal manner, and set patterns to become stereotyped, were it not for the capricious changes of fashion; sometimes slowly developed, at other times, a new fashion suddenly sets in and changes all; the later chasing the earlier out of the field, only to be elbowed aside in its turn. Styles of ornament, as they course each other down the stream of time, invariably leave their high-water marks on the margin, which serve as valuable data for the student; the prevailing styles of decorative and heraldic art, having, like all mundane things, their periods of development, full-blossoming, and decadence, the dates of which, book-plate collectors, aided by dated specimens, arrive at with tolerable certainty.

The prevalence of a particular style, its vogue and duration, will account in a great measure for the family likeness observable in so many book-plates; the chief factors, however, may be set down to the general low state of the art, the paucity of designers and engravers of merit, and the ample supply of the ordinary article—the mechanical craftsman. [Pg 36]

Pure Line Engraving, reproduced by process block.

[Pg 37] As to the history and development of styles in Ex Libris, a reference to the works of the Hon. J. Leicester Warren, J. Paul Rylands, F.S.A., Egerton Castle, M.A., F.S.A., W. J. Hardy, and the pages of the Ex Libris Journal, will find the subject fully and plainly set forth.

A word as to the origin and history of Copper-Plate Engraving. The art of engraving on metal plates, for taking impressions on paper, was first practised by Tommaso Fineguerra, a Florentine goldsmith, about the year 1460. Some writers have claimed the invention for Germany, but it is generally considered that the art was first practised in Italy, and had its origin in the workshops of the goldsmith. An assistant is said to have suggested to Fineguerra the possibility of taking an [Pg 38] impression from an engraved design with ink on moistened paper. The first book printed at Rome was illustrated by the first plate engraving. This work is dated 1478, but was commenced in 1472. Engraving made rapid strides towards excellence in Germany. Albert Dürer was a man whose universality of talent extended the boundaries of every department of art, and carried all to a degree of perfection previously unknown. He had great command of the graver, and carried his plates to a higher state of finish than his Italian contemporaries. He is also believed to have invented the art of etching by corrosion: on examining his etchings, we see that they have all been corroded at one “biting-in,” which sufficiently explains their monotonous appearance, and proves that “stopping-out” was not then understood. To the Dutch and Flemish schools we owe many improvements in the art. The celebrity of the French school dates from the time of Louis XIV. Gerard Audran was [Pg 39] the first engraver who successfully united to any extent the use of the graver and the etching point. The English school of engraving dates [Pg 40] only from the middle of the eighteenth century, previous to which those who practised the art in England were chiefly foreigners. Hogarth [Pg 41] engraved many of his own designs. Francis Vivares introduced the art of landscape etching: he, Woollet, and Brown produced some of the [Pg 42] first landscape engravings extant. Sir Robert Strange excelled in portrait engraving. Of the moderns who have attained eminence in the various branches of the art, the very enumeration of them would lead to needless length, the present purpose being chiefly to describe the processes.

Pure Line Engraving, reproduced by process block.

Line Engraving by William Hogarth,
reproduced by process block.

William Hogarth’s own book-plate.
Line Engraving, reproduced by process block.

### THE VARIOUS MODES OF ENGRAVING ON
COPPER AND STEEL-PLATE.

There are many kinds of engraving on steel and copper for the purpose of printing by the copper-plate press. We will specify those principally in use and indicate their chief characteristics; afterwards, some further explanation may be necessary. It may be here stated that the various processes are of such a technical nature that it would be impossible in a short compass to explain all the details of [Pg 43] execution; we may, however, refer those who desire to pursue the subject further to an excellent little handbook (price one shilling) published by Winsor and Newton,[2] which, as stated in the preface, will, by means of any of the modes of engraving on copper therein treated of, enable anyone “skilled in pen and ink drawing to reproduce their designs with greater delicacy and added depth of effect.” Other books on the subject there are, of greater cost, as Hamerton’s splendid work, but for the amateur the handy little manual just named is an admirable guide.

Transfer, direct from Engraved plate to stone.

[Pg 44]

Pure Line Engraving, reproduced by process block.

Transfer, direct from Engraved plate to stone.

[Pg 45] To one skilled in drawing, and with some leisure and enthusiasm for the work, Etching offers a delightful field for the exercise of the artistic mind. There are no technical difficulties that may not be surmounted by care and patience. The few tools and necessary appliances are not of a costly nature, if we except the copper-plate printing press.

There are different kinds or methods of engraving, the six principal varieties of which need only be considered, namely:—

- (1) Line Engraving.
- (2) Etching.
- (3) Soft-ground Etching.
- (4) Aquatint Engraving.
- (5) Mezzotint Engraving.
- (6) Stipple Engraving.

The distinctive features of all copper-plate and steel-plate engraving consist in this, that the lines or strokes composing the design are cut or ploughed into the surface of the metal with a fine tool termed a graver, etched or corroded out with acid or by other means. A Print is obtained by filling the lines so made with a special ink composed of [Pg 46] a drying oil and colour-pigment. During the process of inking the plate is kept warm, the superfluous ink being wiped off with a coarse muslin rag, and made perfectly clean. The plate, placed in the travelling bed of the copper-plate press, is covered with a sheet of paper slightly damp; on turning the press, it is subjected to such pressure as forces the paper into the lines; by this means the ink is transferred to the paper, and the result is an impression or proof.

Copper-plate Printing Press.

Transfer, direct from Engraved plate to stone.

[Pg 47]

### 1.—LINE ENGRAVING.

The majority of the earlier book-plates are engraved, or cut into the plate entirely with the graver, and may properly be termed line engraving par excellence.

As early examples of this style of work we are enabled to give reproductions of several book-plates, viz., Kress of Kressenstein, by Hans Troschel, 1699, p. 28; the portrait plate of Samuel Pepys, by Robert White, p. 31; two plates engraved by Hogarth, pp. 40-41. The Ex Libris of William Cowper, Clerk of the Parliaments; Edward Loveden Loveden; —— Barrow; and Henʸ Jamˢ Pye, also illustrate the quality of line or graver work alone. The examples interspersed in the text carry their own explanation.

As modern examples of this style we are enabled to give several characteristic varieties—the library interior of W. H. K. Wright, by J. E. Wood, of Plymouth, and a number designed by the writer and [Pg 48] engraved by Marcus Ward & Co., Limited, printed by lithography—all of which will be found useful as keys to the style of handling of graver work alone, and in combination with etching.

Among the chief exponents of the art may be mentioned the name of C. W. Sherborn, who is facile princeps as an engraver of heraldic subjects. One of his smaller works, engraved in pure line, appears facing page 27, the dainty crest plate of R. Day, F.S.A., printed direct from the copper-plate; a favourite old toast, in playful allusion to the wings in the crest, doing duty as a motto.

### 2.—ETCHING.

This method admits greater freedom of handling than graver work. The design is drawn through a resisting ground with the etching point, and the exposed lines on the surface of the copper corroded to the requisite depth with aquafortis, the finishing of the work being usually done with the graver.

Transfer, direct from Engraved plate to stone.

[Pg 49]

Etching on Copper reproduced by process block.

From the collection of W. H. K. Wright.

[Pg 50] Machine ruling or tinting is now much used in conjunction with line engraving and etching, for the even tints of skies and level surfaces in pictorial work, and for the symbolical lines denoting tinctures in heraldry, of which several examples are given.

Steel-plates were used for engraving very fine work, or when large numbers of copies were required to be printed from the plate. Any advantage over copper which steel formerly possessed is now neutralised by the process known as steel facing, that is, coating the copper plate with an electro deposit of iron.

Copper-plate printing, as it is termed, though giving the most perfect result, is slow and tedious, and necessarily costly. A much speedier method of printing—by Lithography—is now much used instead, transfers from the engraved plate being put on the lithographic stone and printed therefrom, the original plate being retained intact. (See examples under Lithography). [Pg 51]

Two Etchings on Copper by Bewick, reproduced by process block.

From the collection of W. H. K. Wright.

[Pg 52] Some early examples of etched plates are given. The urn design of Charles Bragge, Armorial Landscape, and Bewickian Landscape show the character and handling of etched work as distinguished from line engraving. Other examples illustrate the combination of Line, Etching, and Machine Ruling work.

### 3.—SOFT-GROUND ETCHING.

A very charming style of work which was much used by Bartolozzi and other engravers of his time, but now gone entirely out of use. A suitable book-plate engraved in this manner not turning up in time, the present fine example of the style was selected to illustrate the character of the work, which bears a close resemblance to a chalk drawing, and on that account offers considerable difficulties in the way of reproduction by the half-tone process. The result is, however, successful in a remarkable degree in translating the peculiar texture of the original.

Transfer, direct from Engraved plate to stone.

[Pg 53]

Two Etchings on Copper by Bewick, reproduced by process block.

From the Collection of W. H. K. Wright.

[Pg 54] The allegorical device represents the turret-crowned goddess Cybele, “mother of a hundred gods,” standing upon an isolated rock in the sea, holding out an olive-branch, and with her attribute, the rudder, as guide and director of the destinies of cities and states; youthful figures representing the Arts and Sciences—which are the glory of a State—are disporting themselves in the clouds.

Though not originally intended for a book-plate, a friend is desirous of adopting it, with the motto from Virgil, “Fato prudentia major”—to intimate that, in his opinion, prudence is greater than fate.

### 4.—AQUATINT ENGRAVING.

A style of work having all the appearance of a china ink drawing, and frequently used by artists in conjunction with etching, to give body and consistency to the tints. An admirable example of this combination of etching and aquatint is the charming book-plate of the Hon. Leicester Warren, by W. Bell Scott, well known to collectors. It does not, however, lend itself well to reproduction.

Transfer, direct from Engraved plate to stone.

[Pg 55] The texture, which may be of various degrees of fineness, is produced on the plate by a solution of resin (dissolved in pure spirit), which is poured over the surface; as the spirit evaporates it leaves the resin in minute isolated particles adhering to the plate. The design is traced or transferred upon it, the highest lights “stopped out” with engravers’ varnish. The etching (or biting-in with acid) is then proceeded with; repeated stoppings out and etchings are made as the deeper shades are attained.

### 5.—MEZZOTINT ENGRAVING.

Produced by roughening the surface of the plate by a rocking tool, and the lights and shades attained by scraping and burnishing. Seldom used for small work, but largely used combined with Nos. 1 and 2 for prints [Pg 56] and pictures. The small French print of the Virgin and Child, reproduced by half-tone process block, represents fairly well the character of the work. (See example under “Half-tone Process Blocks.”)

### 6.—STIPPLE ENGRAVING.

Performed with the graver or other tool, which is so managed as to produce the tints by small dots. This method is much used for statuary and for portraits particularly, the rest of the picture being generally executed by some of the other methods, Nos. 1 and 2 especially.

Transfer, direct from Engraved plate to stone.

[Pg 57]

Etching on Copper, reproduced by process block.

Lithographic Printing Press.

[Pg 58]

## LITHOGRAPHY.

Lithography, as one of the modern arts, dates only from about the end of the last century. The inventor, Aloys Senefelder, the son of an actor, was born at Munich in 1771, and died there on the 26th February, 1834. Intended for the profession of the Law, he, on the death of his father, was obliged to retire from the University.

Drawn on transfer paper and transferred to stone direct.

[Pg 59] Thrown on his own resources at the age of eighteen, he turned to his father’s profession, but met with little success. Writing for the stage, he found difficulty, owing to his poverty, in getting his writings published, and it was in trying to find out some ready process to attain this end that he arrived at what we now term the Art of Lithography. Senefelder lived to perfect his art to a high degree, and to see it brought into general use, but without bringing much profit to himself. Since his time many advances have taken place, and new developments in various directions, as in the beautiful art of chromo-lithography and photo-lithography.

The term Lithography is derived from the Greek, lithos, a stone, and grapho, to write. Lithographic stone is a species of limestone, the best qualities of which are obtained from the quarries at Solenhofen, near Munich, and from Papenheim, on the Danube. The stones are cut into slabs or blocks of various sizes to suit the work required; to print an octavo page, quarto, etc., up to sixty inches by forty, and even [Pg 60] larger. The thickness varies from an inch and a half in the smaller, to four or five inches in the larger sizes. The stones are ground perfectly level with sand and water, and finished off with a fine stone until a perfectly smooth polished surface is produced, when it is ready to receive the drawing, or to have transferred to its surface a drawing or writing made upon specially prepared paper (lithographic transfer paper). For chalk or crayon drawings, the smooth surface of the stone is grained with sifted silver sand, which gives a beautifully even granular texture, and the drawing is made upon it with lithographic chalk. For drawing upon the smooth stone, or upon transfer paper, lithographic ink is used.

The principle underlying the process of Lithography is simply this:—The nature of the stone is such that it retains with great tenacity the resinous and oily substances contained in the ink or the crayon employed to form the design. The lithographic stone also absorbs water freely; this, combined with the peculiar affinity between resinous substances and their mutual power of repelling water, causes the ink on the printing roller to adhere to the design and to leave untouched the damp surface of the stone.

Drawn on transfer paper and transferred to stone direct.

[Pg 61] The process of Lithographic Printing is as follows:—After the drawing on the litho. stone is completed, it receives a wash of dilute acid and gum arabic, and this, by removing the alkali from the ink, leaves the design on it in a permanent form, at the same time that it etches away a minute portion of the surface of the stone, and renders it more absorbent of water. After etching, all trace of the acid is removed with a sponge and water, the stone is rubbed over with a damp muslin cloth to equalise the moisture upon the surface, the lithographic roller charged with printing ink is passed over the surface, the lines of the design alone taking ink; the paper is then [Pg 62] laid upon the stone, and a copy is obtained by means of the lithographic press. The damping of the stone and inking is repeated for every impression.

Lithographic Writing and Drawing Ink and Lithographic Crayons for chalk drawing on stone, are similar in composition, but different in proportions, suited to the particular kind of work, white wax, shell-lac, hard soap, tallow, and lamp black being the chief ingredients. For writing and drawing all kinds of line work on stone or transfer paper, the ink is made in sticks, and rubbed down with water to a proper consistency for use, and used with a pen or sable pencil. For chalk drawings upon a grained stone, the ink is cast into the form of crayons, and used in a port-crayon for convenience in drawing, sharpening the point as required.

Chalk Drawing on Stone is rarely used for such small work as book-plates. We need not therefore more particularly refer to it, than to say that excellence in this department of Lithography may be attained more readily than in fine-line work, for which constant practice, and a very delicate handling of the implements, the lithographic pen and fine sable pencil, is required.

Drawn on transfer paper and transferred to stone direct.

[Pg 63] The technical difficulties to be overcome in Lithography are very great; to the unpractised they seem insuperable: the magic of handling acquired by long-continued practice in the use of the materials, as seen in good examples, exhibits a degree of technical skill which the amateur may not hope to rival. To draw with the pen or small sable pencil with the requisite degree of fineness of line of the expert, and with the precision and apparent freedom of the accomplished artist, is a thing of difficult attainment. This is a disadvantage to artists generally, who are obliged to entrust the translation of their drawings to the professional lithographer—not always with a satisfactory result(!) [Pg 64]

Grained or Textured Paper, of which there are many varieties specially made with a chalky surface for photo-lithography, are now much used, on which the artist makes his drawing in litho-chalk or suitable black lead pencil. As the knife point may be used to scrape out lights on the chalky surface, it admits of very effective work for pictorial illustrations. A photo-litho transfer is then put to stone, or a process block made from it, as may be required. Drawings made on this prepared textured paper with lithographic chalk may also be transferred to stone direct, and printed from. Extreme beauty and fineness are, however, gained by the photo-reduction.

Very beautiful Pictorial and Heraldic Ex Libris have been executed by the lithographic process, hardly to be distinguished from plate engraving.

Engraved Plates may have transfers taken from them and printed from stone. A number of examples, with explanatory titles, are given of the various modes of lithographic and photo-lithographic reproduction.

Drawn on transfer paper and transferred to stone direct.

[Pg 65]

### CHROMO-LITHOGRAPHY.

Some very dainty examples of Ex Libris emblazoned in heraldic tinctures are met with, very charming in their way, principally German ones. Colour in the heraldry of book-plates has not found the same favour in this country as on the Continent; for what reason it is hard to understand. Through the courtesy of Mr. R. S. Mansergh, Friarsfield, co. Tipperary, we are enabled to print as a frontispiece the plate newly designed by the writer, and executed by Messrs. Marcus Ward & Co., of Belfast.

### PHOTO-LITHOGRAPHY.

Photo-lithography is now so largely employed for the reproduction of all classes of work that a few words in explanation of it may be very desirable. The process is of a somewhat technical nature, but simplicity itself when understood! It is founded upon the fact that gelatine, by the addition of a certain chemical, is rendered insoluble on exposure to light. [Pg 66]

A negative photograph from the original drawing in black lines having been taken by the wet or collodion plate, it is intensified to the required degree, so that the lines of the design appear perfectly clear upon a dense, opaque, black film. It is then “exposed” in the printing frame, upon paper that has been coated (in the dark) with the prepared gelatine—now extremely sensitive to light. Taken out of the printing frame in the dark room, the exposed print (which barely shows any trace of the design at this stage) is then covered with a thin film or coating of printers’ transfer ink. The lines exposed to the light have been rendered insoluble, while the white ground of the design protected by the negative is still in a soluble condition. Floated in a bath of warm water, the soluble gelatine (not acted on by the light), with its coating of ink, is washed away—the insoluble lines of the design alone remaining, coated with printers’ transfer ink. This “photo-transfer” is then ready to be put down to the lithographic stone and printed from, or it may be transferred to a polished zinc plate, and etched to the requisite depth as a block for type printing.

Drawn on stone direct, with mechanical ruling added.

[Pg 67]

### DRAWING FOR PHOTO-LITHO, AND FOR
PROCESS LINE-BLOCKS.

The invention of photo-lithography enables the artist to make his own drawings or designs in black and white on a larger scale (usually one-third or one-half larger than required), which will be photo-litho’d down to the size required, thus preserving intact every touch and flexture of line in the original, and, by the reduction, gaining a fineness of line and beauty of finish which the artist could not himself produce on the reduced size. Machine Ruling may afterwards be transferred into the design when it is upon the stone, as in some of the designs in the accompanying examples.

“Process blocks,” which reproduce so admirably all kinds of drawings and engravings, are, when carefully printed, sometimes very difficult to detect from direct lithographs. [Pg 68]

Ulster King of Arms.

Pen and Ink Drawing by Rev. Wm. FitzGerald,
reproduced by process block. Much reduced.

[Pg 69]

## PROCESS BLOCKS.

### LINE WORK.

There are quite a number of processes that have been brought into use with more or less success, as Graphotype, Dallas-type, etc., to which it is not necessary to refer, as for all practical purposes Zinc Etching holds the field against all others, either for Half-tone Blocks, or for Line-Blocks of every kind, of which last a number of examples are here given, with an explanatory title to each specimen.

For work of the very finest kind, the Photogravure or Heliogravure, printed by the copper-plate press, bears the palm, but it has the disadvantage of being very expensive. Those desirous of knowing more fully concerning the various processes in use may be referred to a very excellent volume in the “Book Lovers’ Library”—“Modern Methods of Illustrating Books,” by H. Trueman Wood, M.A., Secretary to the Society of Arts, and published by Elliot Stock. [Pg 70]

Pen and Ink Drawing, reproduced by process block.
Slightly reduced.

Pen and Ink Drawing reproduced by
Photo-lithography.

[Pg 71] These modern methods provide a most important and valuable means of producing illustrations for printing purposes. By their aid, any photograph, drawing, design, or engraving of any kind can be translated into a block, and with such success that, with suitable subjects, it is often hardly possible to tell the original from the copy; and not only do they enable surface blocks to be produced with great rapidity and at slight cost, but they give blocks capable of producing effects which could not be obtained at all by wood engravings, or, if at all, only at great expense.

Many artists have hailed with delight the process of Zinc Etching, as by its means they obtain a perfect fac-simile of their work, more especially pen and ink drawing, which could never be reproduced by any other method with the same accuracy and delicacy of finish which the zinc process gives, and which could not by wood engraving be an absolute fac-simile. [Pg 72]

Pen and Ink Drawing,
reproduced by process block.
Slightly reduced.

Pen and Ink Drawing reproduced by
Photo-lithography.

[Pg 73]

Pen and Ink Drawing, reproduced by process block.
(Same size.)

Mr. Carl Hentschel, head of an eminent firm of photo-etchers, to whom we applied for information upon certain points in the manipulation of his process, courteously offered some very interesting statements as to the development of zinc etching. He says the process of Zinc Engraving was introduced into England about thirty years ago, but really did not “catch on,” as the Yankees would say, for twenty years after; nor was [Pg 74] there any real value attached to it from a commercial point of view until about twelve years ago, when, as Mr. Hentschel assures us, the system he adopted rendered it possible to have blocks of all kinds for newspapers, books, magazines, and journals of every description produced in such time that their delivery could be relied upon for the most urgent publication, and, only then, the vast possibilities of the zinc process began to dawn upon publishers, and soon the method was gradually adopted for all purposes of engraving. Some idea of the extent to which it is made use of may be gathered from the fact that [Pg 75] this firm alone delivers weekly about three thousand blocks for various publications throughout the country, and even to far-off India, where the plates of whole volumes of educational works have been despatched by this enterprising firm. To keep pace with the requirements of the times it has been found necessary recently to add largely to the facilities for the execution of half-tone blocks, using engine power to the extent of forty horse for the production of the electric light, essential for this branch of the business, so that in this respect they are practically independent of sunlight. In cases of emergency it is no unusual thing to deliver half-tone blocks in five to seven hours, and Line work, from transfers, one and half hours, and in the case of having to photo the subject, two and half to three hours. This would have been impossible under the old system, trusting to daylight, and this fact, coupled with the cheaper rate of cost, has given an impetus to illustrated journalism that could hardly have been dreamt of under the old regime. [Pg 76]

Pen and Ink Drawing, reproduced by process block.
Slightly reduced.

[Pg 77] Under the head of photo-lithography, the initiatory stage in the making of what are termed “Process Blocks” was explained, namely, the making of photo-transfer from the original drawing—in printer’s ink—for transference to the lithographic stone and printed form. The metal Zinc possesses the same or similar properties as lithographic stone, and may be used to print from in the same way. The term Zincography is applied to the process, though practically it is the same as lithography. [Pg 78]

Drawn in pen and ink, reproduced by process block.

[Pg 79] To convert the design upon the zinc plate into a relief block to print with type is only one step farther—to so protect the lines of the design on the zinc plate, as to resist the corrosive action of acid, and by etching the plate, produce a relief block. For this purpose, a resinous or bituminous substance is introduced into the composition of the printing ink. Here, then, we have the lines of the design in an acid-resisting material upon the surface of a metal plate exceedingly susceptible to the action of acids. If the prepared plate is now placed in an acid bath, the entire surface of the zinc, except the protected lines, will become etched, or dissolved away, leaving the design in its integrity, with the lines standing up in relief: the etched plate has now only to be mounted upon wood to the height of type to be ready for the printer’s use. [Pg 80]

Pen and Ink Drawing, reproduced by process block.

Pen and Ink Drawing reproduced by Photo-lithography.

[Pg 81] Such is a brief outline of the process in the production of Line Blocks. The design may be put on the metal plate in any of the following ways:—

- (a) By direct drawing on the zinc plate.
- (b) By a drawing on transfer paper to zinc or stone.
- (c) By transference of a photo-transfer.
- (d) By transfer from an engraved plate.
- (e) By transfer from a lithographic stone.
- (f) By direct photography upon zinc.

The most perfect work is said to be obtained by the latter method. There are many technical difficulties to be encountered in working the process, difficulties which for twenty years kept it at the experimental stage, and of little practical utility, as, for instance, after etching the plate for a short time the acid has a tendency to bite laterally as well as vertically, and so undermine and weaken the lines intended to be left standing. This is obviated by some photo etchers in using certain chemicals, and others by an ingenious manner in the working by etching in stages. This is done by re-inking and dusting with bitumen, heating the plate after each “etching,” which has the effect of melting and spreading the resinous or bituminous ink on the face, and slightly down the sides of the lines. Successful work is only attained by attention to the various delicate technical manipulations, which only experience can give. [Pg 82]

Pen and Ink Drawing, reproduced by process block.

Reproduced by half-tone process block,
from a Monochrome Sketch,
reduced in size.

[Pg 83]

### HALF-TONE PROCESS BLOCKS.

The subject, whether it is a drawing, engraving, painting, or a photo print, must in each case be photographed to obtain upon the negative the texture which is the means of producing the gradations of light and dark we find in the finished block. The theory is simple enough, but the practice is extremely difficult, and one requiring great skill and [Pg 84] care. A glass screen having cross lines ruled upon it, with perfect mechanical regularity (about seventy lines to the inch for large work, up to two hundred lines to the inch for very fine half-tone blocks, as may be best suited to the subject in hand). The screen is fixed in the camera between the lens and the negative to be exposed. The fine black lines of the screen are reproduced upon the negative as white lines, [Pg 85] breaking up the picture into a series of minute square dots, of varying size according to the light and shade of the original picture. A photo-transfer is then taken as previously explained. (In Hentschel’s process the secret of the prepared transfer paper is in the possession of Mr. Hentschel solely.) After being transferred to the zinc, and manipulated with certain chemicals, the plate is gradually etched until a sufficient depth has been obtained. It is then trimmed and mounted type height ready for the printer.

Pen and Ink Drawing, reproduced by process block.

[Pg 86]

Original size.

Pen and Ink Drawing,
reproduced by process block in three sizes.

[Pg 87]

### PEN AND INK DRAWING.

Drawings for reproduction by the modern processes of photo-lithography and photo-etching may be prepared in a variety of ways. The most frequently used is termed Pen and Ink Drawing (often mistakenly called “etching,” which is engraving by means of an acid). This class of work is the most popular of all, and the most easily got at by artists and amateurs; it is translated with much greater ease, and at less cost, than photographs or shaded drawings of any kind. As the term indicates, it is executed with the pen; many artists, however, have a predilection for the brush (a fine sable pencil), which, though it requires considerable practice to master its use, becomes in masterly hands a valuable instrument, capable of greater and more varied effects than the pen. Good black ink, and smooth white paper or cardboard, are the essentials. Much may be said on the style or modes of different artists in drawing, the kind or quality of the ink, the pens and paper to be used. The relative values of thick and[Pg 88] thin, open and close lines, the direction of the lines, etc., in producing the varied character and quality of good expressive drawing; the various textures of surfaces—roughness, smoothness, etc.—have all to be considered, more especially if the drawing is made upon a larger scale, to be reduced in the photo-etching process of translation. We heartily commend the shilling handbook on Pen and Ink drawing published by Winsor and Newton. It is an excellent introduction to the art; it gives full instructions on the best means of working, and the materials to be used.[3]

Club Device and Ex Libris.

Pen and Ink Drawing, reproduced by process block.

Reproduced by half-tone process block,
from an Aqua-Tint engraving, same size.

[Pg 89] For Half-tone Shaded Blocks the design may be executed in washes as a china ink drawing, or in any other way. The illustrations are reproductions from various kinds of originals, as explained under each example.

Messrs. Carl Hentschel & Co., 182-3 Fleet Street, have been good enough to prepare several examples to illustrate the half-tone process; each block having been made from an original executed in a different way, as indicated by the explanatory title; and may be considered rather severe tests of what the process is capable. For these favours we are much obliged; we tender also our thanks for their kindness and courtesy in supplying much of the foregoing information. [Pg 90]

Pen and Ink Drawing, reproduced by process block.

[Pg 91]

## HINTS TO COLLECTORS
OF EX LIBRIS.

### To distinguish how a book-plate
may have been produced.

A lithograph or a photo-lithograph may be distinguished from a woodcut, or from a copper engraving, by the following: By the quality of the lines, whether cut with the graver or etched upon copper; drawn with the pen or with the fine sable pencil. Each has a character of handling and manner of its own by which it may be recognised. A little observation of admitted examples with the aid of a strong magnifying glass will generally resolve this. [Pg 92]

EX LIBRIS.

Reproduced by half-tone process block, from
Coloured Design for Stained Glass Window.

[Pg 93]

### THE DIFFERENCE IN ENGRAVED OR
CUT LINES, AND ETCHED LINES.

Lines cut with the graver are invariably smooth and even, and have a clear silvery appearance; in isolated lines or cuts it will be observed that the beginning of the lines are finer where the graver has entered than where it stops. Etched lines, on the contrary, do not possess the same smooth-edged rigid character as those cut with the graver; and where greater strength of line is obtained it is by deeper etching with the acid bath, and in this the difference in the quality of line is more perceptible.

### TO DISTINGUISH AN IMPRESSION
FROM PLATE.

In a plate engraving the lines are slightly in relief (and, if strongly engraved, or the paper thin, observable on the back). A sensitive finger will detect the stronger raised lines of the engraving. The mark of the plate, unless cut off, also betrays it; the engraved plate by Mr. Sherborn, facing page 27, will illustrate this. [Pg 94]

### TO DISTINGUISH A WOODCUT,
OR LINE PROCESS BLOCK.

In a block the lines of the design are indented slightly into the paper, which shows itself on the back of the print (unless thoroughly rolled out under heavy pressure). Close observation with the magnifying glass will show the edges of the lines to be slightly rough—by the ink from the face of the line being squeezed over the edge; in good printing this is not so apparent. A weakness with nearly all process blocks is that the edges of fine tints and outlying fine lines are apt to print heavier than they should, unless very carefully worked.

### TO DISTINGUISH A LITHOGRAPH.

In a lithograph the surface of the paper is perfectly smooth, and not indented in any way. The examples of engraved plates printed from stone, and the litho. and photo-litho’s printed in brown ink, will serve to illustrate the qualities of lithography. Unless well printed, the fine lines are apt to show weak and rotten, or to have become thick and blurred, either in transferring to the stone or by too much ink on the printing roller.

FATO PRUDENTIA MAJOR.

Ex Libris VINICOMBE BEY,
Colonel d’ Artillerie Tophané, Constantinople.

Example of soft-ground etching—Reproduced
by half-tone process block.

[Pg 95]

## “AU REVOIR.”

Having now rehearsed, I hope clearly and concisely, the various modes by which Ex Libris are and have been produced, and having revealed as many trade secrets as the limited space at command would allow, I beg to thank the Council of the Ex Libris Society for permission to reprint from the pages of the Journal the series of articles on the subject—now somewhat expanded—and for the use of the blocks by which they were illustrated. To Mr. W. H. K. Wright, F.R.Hist.Soc., the able Editor and Secretary of the Ex Libris Society (to whom all collectors are infinitely indebted), my thanks are due for his valued aid and counsel; and on whose shoulders I have now laid the further obligation of a preface. As a special favour I have requested his “library interior” plate to appear. A similar favour I have desired from Arthur Vicars, F.S.A., Ulster King of Arms, to whom I dedicate this little book. With the exception of these two “library interiors” and the crest plate of R. Day, F.S.A., [Pg 96] by Sherborn, all the modern Ex Libris designs here printed have been made by, or under the superintendence of, the writer, and executed by Marcus Ward & Co., Limited, whom I beg to thank most heartily for their kind co-operation, particularly in printing the lithographed specimens, and the use of additional blocks. I have also to thank several personal friends who have been good enough to lend me their copper-plates and process blocks.

John Vinycomb, m.r.i.a.

Riverside, Holywood, co. Down, 1894.

THE

Journal

OF THE

Ex Libris Society,

PUBLISHED MONTHLY,

Price, 1s. 6d.  Post Free, 1s. 9d.

ALSO, |  |
VOLUME I. | — | Out of Print
VOLUME II. | — | Out of Print
VOLUME III. | Price, 21s. | Post Free, 21s. 8d.

Cases for the above Volumes—

Price, 1s. 6d.  Post Free, 1s. 9d.

ADAM AND CHARLES BLACK,

SOHO SQUARE, LONDON.

Dated Book-Plates

(Ex Libris),

With a Treatise on their Origin and Development.

BY
WALTER HAMILTON,

Chairman of Council of the Ex Libris Society; Vice-President
of the Société Française des Collectionneurs d’Ex Libris.

With Numerous Illustrations.

A list of Dated Plates prior to 1700 appears in Part I., with fac-similes of Ex Libris specially selected as typical examples of early work.

Part II. will contain Dated Plates of the 18th century.

Part III. will contain Dated Plates of the 19th century.

The work will be printed on paper of the same size as the Journal of the Ex Libris Society, so as to range with it.

The price of each part will be Seven Shillings and Sixpence net. Post free, 7s. 11d.

Part I. is now ready. Parts II. and III. will be issued very shortly, as all the materials are ready for the press.

ADAM AND CHARLES BLACK,

SOHO SQUARE, LONDON.

Book-Plate Annual

AND

ARMORIAL YEAR BOOK,

1894.

Edited by JOHN LEIGHTON, F.S.A.
Price, 2s. 6d.   Post Free, 2s. 9d.

Contents—

1.—Half Title, the Author, the Printer, the Bookbinder, and the lover of Books.

2.—Memorandum Sheet for the entry of Loans and Exchanges.

3.—The Ex Libris of the Duke of York and Princess. (By gracious permission.)

4.—Description of the Royal Wedding Book-plate. By Arthur Jewers, F.S.A.

5.—Portrait of the Great Master of Symbolical Heraldry, Albert Dürer.

6.—Should Wales have a place on the Royal Standard of England.

7.—Suggestions for a Welsh Order of Knighthood. The Collar and Jewel of St. David.

8.—Cambria upon the Currency in the fourth quarter.

9.—The Library, Books and Bindings. Their Restoration and Preservation.

10.—How to keep Ex Libris under any classification or arrangement.

11.—The Process of Binding. A Book from the Sheets to the Volume.

12.—Taxes upon Vanity. Armorial, Servants, Horses, and Carriages.

13.—Arms of Participation. An Economy in a high Luxury.

14.—Rebinding Old Books of value; what should be done?

15.—The Find of the Year. The Virginian Book-plate confirmed in America.

16.—Cut and come again. The Trimming of Books and Cutting Down.

ADAM AND CHARLES BLACK, SOHO SQUARE, LONDON.

THE

DRYBURGH EDITION

OF THE

Waverley Novels.

With 250 Page Illustrations, specially Drawn for this Edition
by the well known Artists whose names are given below, and
engraved on wood by Mr. J. D. COOPER.
In Twenty-five Volumes.

Crown 8vo, Cloth. Price, 5s. each.

CHARLES GREEN |  | WAVERLEY.
GORDON BROWNE |  | GUY MANNERING.
PAUL HARDY |  | THE ANTIQUARY.
LOCKHART BOGLE |  | ROB ROY.
WALTER PAGET |  | BLACK DWARF.
LOCKHART BOGLE | LEGEND OF MONTROSE.
FRANK DADD, R.I. |  | OLD MORTALITY
WILLIAM HOLE, R.S.A. |  | HEART OF MIDLOTHIAN.
JOHN WILLIAMSON |  | BRIDE OF LAMMERMOOR.
GORDON BROWNE |  | IVANHOE.
JOHN WILLIAMSON |  | THE MONASTERY
JOHN WILLIAMSON |  | THE ABBOT.
H. M. PAGET |  | KENILWORTH.
W. H. OVEREND |  | THE PIRATE.
GODFREY C. HINDLEY |  | FORTUNES OF NIGEL.
STANLEY BERKELEY |  | PEVERIL OF THE PEAK.
H. M. PAGET |  | QUENTIN DURWARD.
HUGH THOMSON |  | ST. RONAN’S WELL.
GEORGE HAY, R.S.A. |  | REDGAUNTLET.
GODFREY C. HINDLEY |  | THE BETROTHED.
HIGHLAND WIDOW.
GODFREY C. HINDLEY |  | THE TALISMAN.
STANLEY BERKELEY |  | WOODSTOCK.
C. M. HARDIE, A.R.S.A. |  | FAIR MAID OF PERTH.
PAUL HARDY |  | ANNE OF GEIERSTEIN.
GORDON BROWNE |  | COUNT ROBERT OF PARIS.
PAUL HARDY |  | THE SURGEON’S DAUGHTER.
WALTER PAGET | CASTLE DANGEROUS.

ADAM AND CHARLES BLACK, SOHO SQUARE, LONDON.

Footnotes:

[1] Jackson’s “History and Practice of Wood Engraving”; Firmin Didot’s “Essai sur l’Histoire de la Gravure sur Bois”; “The Book, its Printers, Illustrators, and Binders,” by Henri Bouchot; “Wood Engraving: a Manual of Instruction,” by W. J. Linton.

[2] “The Art of Etching explained and illustrated, with remarks on the allied processes of Dry-point, Mezzotint, and Aquatint.” By H. R. Robertson, Fellow of the Society of Painter-Etchers; Author of “Life on the Upper Thames,” etc. Winsor and Newton, Limited, 38 Rathbone Place, London.

[3] “The Art of Pen and Ink Drawing, commonly called Etching.” By H. R. Robertson, Fellow of the Society of Painter-Etchers, Author of “The Art of Etching,” etc. Winsor & Newton, Limited, London.

Transcriber’s Notes:

Antiquated spellings were not preserved.

The illustrations have been moved so that they do not break up paragraphs and so that they are next to the text they illustrate.

Typographical errors have been silently corrected.

*** END OF THE PROJECT GUTENBERG EBOOK ON THE PROCESSES FOR THE PRODUCTION OF EX LIBRIS (BOOK-PLATES) ***
Updated editions will replace the previous one—the old editions will be renamed.
Creating the works from print editions not protected by U.S. copyright law means that no one owns a United States copyright in these works, so the Foundation (and you!) can copy and distribute it in the United States without permission and without paying copyright royalties. Special rules, set forth in the General Terms of Use part of this license, apply to copying and distributing Project Gutenberg™ electronic works to protect the PROJECT GUTENBERG™ concept and trademark. Project Gutenberg is a registered trademark, and may not be used if you charge for an eBook, except by following the terms of the trademark license, including paying royalties for use of the Project Gutenberg trademark. If you do not charge anything for copies of this eBook, complying with the trademark license is very easy. You may use this eBook for nearly any purpose such as creation of derivative works, reports, performances and research. Project Gutenberg eBooks may be modified and printed and given away—you may do practically ANYTHING in the United States with eBooks not protected by U.S. copyright law. Redistribution is subject to the trademark license, especially commercial redistribution.
START: FULL LICENSE

## THE FULL PROJECT GUTENBERG LICENSE

PLEASE READ THIS BEFORE YOU DISTRIBUTE OR USE THIS WORK
To protect the Project Gutenberg™ mission of promoting the free distribution of electronic works, by using or distributing this work (or any other work associated in any way with the phrase “Project Gutenberg”), you agree to comply with all the terms of the Full Project Gutenberg™ License available with this file or online at www.gutenberg.org/license.
Section 1. General Terms of Use and Redistributing Project Gutenberg™ electronic works
1.A. By reading or using any part of this Project Gutenberg™ electronic work, you indicate that you have read, understand, agree to and accept all the terms of this license and intellectual property (trademark/copyright) agreement. If you do not agree to abide by all the terms of this agreement, you must cease using and return or destroy all copies of Project Gutenberg™ electronic works in your possession. If you paid a fee for obtaining a copy of or access to a Project Gutenberg™ electronic work and you do not agree to be bound by the terms of this agreement, you may obtain a refund from the person or entity to whom you paid the fee as set forth in paragraph 1.E.8.
1.B. “Project Gutenberg” is a registered trademark. It may only be used on or associated in any way with an electronic work by people who agree to be bound by the terms of this agreement. There are a few things that you can do with most Project Gutenberg™ electronic works even without complying with the full terms of this agreement. See paragraph 1.C below. There are a lot of things you can do with Project Gutenberg™ electronic works if you follow the terms of this agreement and help preserve free future access to Project Gutenberg™ electronic works. See paragraph 1.E below.
1.C. The Project Gutenberg Literary Archive Foundation (“the Foundation” or PGLAF), owns a compilation copyright in the collection of Project Gutenberg™ electronic works. Nearly all the individual works in the collection are in the public domain in the United States. If an individual work is unprotected by copyright law in the United States and you are located in the United States, we do not claim a right to prevent you from copying, distributing, performing, displaying or creating derivative works based on the work as long as all references to Project Gutenberg are removed. Of course, we hope that you will support the Project Gutenberg™ mission of promoting free access to electronic works by freely sharing Project Gutenberg™ works in compliance with the terms of this agreement for keeping the Project Gutenberg™ name associated with the work. You can easily comply with the terms of this agreement by keeping this work in the same format with its attached full Project Gutenberg™ License when you share it without charge with others.
1.D. The copyright laws of the place where you are located also govern what you can do with this work. Copyright laws in most countries are in a constant state of change. If you are outside the United States, check the laws of your country in addition to the terms of this agreement before downloading, copying, displaying, performing, distributing or creating derivative works based on this work or any other Project Gutenberg™ work. The Foundation makes no representations concerning the copyright status of any work in any country other than the United States.
1.E. Unless you have removed all references to Project Gutenberg:
1.E.1. The following sentence, with active links to, or other immediate access to, the full Project Gutenberg™ License must appear prominently whenever any copy of a Project Gutenberg™ work (any work on which the phrase “Project Gutenberg” appears, or with which the phrase “Project Gutenberg” is associated) is accessed, displayed, performed, viewed, copied or distributed:

> This eBook is for the use of anyone anywhere in the United States and most other parts of the world at no cost and with almost no restrictions whatsoever. You may copy it, give it away or re-use it under the terms of the Project Gutenberg License included with this eBook or online at www.gutenberg.org. If you are not located in the United States, you will have to check the laws of the country where you are located before using this eBook.

1.E.2. If an individual Project Gutenberg™ electronic work is derived from texts not protected by U.S. copyright law (does not contain a notice indicating that it is posted with permission of the copyright holder), the work can be copied and distributed to anyone in the United States without paying any fees or charges. If you are redistributing or providing access to a work with the phrase “Project Gutenberg” associated with or appearing on the work, you must comply either with the requirements of paragraphs 1.E.1 through 1.E.7 or obtain permission for the use of the work and the Project Gutenberg™ trademark as set forth in paragraphs 1.E.8 or 1.E.9.
1.E.3. If an individual Project Gutenberg™ electronic work is posted with the permission of the copyright holder, your use and distribution must comply with both paragraphs 1.E.1 through 1.E.7 and any additional terms imposed by the copyright holder. Additional terms will be linked to the Project Gutenberg™ License for all works posted with the permission of the copyright holder found at the beginning of this work.
1.E.4. Do not unlink or detach or remove the full Project Gutenberg™ License terms from this work, or any files containing a part of this work or any other work associated with Project Gutenberg™.
1.E.5. Do not copy, display, perform, distribute or redistribute this electronic work, or any part of this electronic work, without prominently displaying the sentence set forth in paragraph 1.E.1 with active links or immediate access to the full terms of the Project Gutenberg™ License.
1.E.6. You may convert to and distribute this work in any binary, compressed, marked up, nonproprietary or proprietary form, including any word processing or hypertext form. However, if you provide access to or distribute copies of a Project Gutenberg™ work in a format other than “Plain Vanilla ASCII” or other format used in the official version posted on the official Project Gutenberg™ website (www.gutenberg.org), you must, at no additional cost, fee or expense to the user, provide a copy, a means of exporting a copy, or a means of obtaining a copy upon request, of the work in its original “Plain Vanilla ASCII” or other form. Any alternate format must include the full Project Gutenberg™ License as specified in paragraph 1.E.1.
1.E.7. Do not charge a fee for access to, viewing, displaying, performing, copying or distributing any Project Gutenberg™ works unless you comply with paragraph 1.E.8 or 1.E.9.
1.E.8. You may charge a reasonable fee for copies of or providing access to or distributing Project Gutenberg™ electronic works provided that:

- • You pay a royalty fee of 20% of the gross profits you derive from the use of Project Gutenberg™ works calculated using the method you already use to calculate your applicable taxes. The fee is owed to the owner of the Project Gutenberg™ trademark, but he has agreed to donate royalties under this paragraph to the Project Gutenberg Literary Archive Foundation. Royalty payments must be paid within 60 days following each date on which you prepare (or are legally required to prepare) your periodic tax returns. Royalty payments should be clearly marked as such and sent to the Project Gutenberg Literary Archive Foundation at the address specified in Section 4, “Information about donations to the Project Gutenberg Literary Archive Foundation.”
- • You provide a full refund of any money paid by a user who notifies you in writing (or by e-mail) within 30 days of receipt that s/he does not agree to the terms of the full Project Gutenberg™ License. You must require such a user to return or destroy all copies of the works possessed in a physical medium and discontinue all use of and all access to other copies of Project Gutenberg™ works.
- • You provide, in accordance with paragraph 1.F.3, a full refund of any money paid for a work or a replacement copy, if a defect in the electronic work is discovered and reported to you within 90 days of receipt of the work.
- • You comply with all other terms of this agreement for free distribution of Project Gutenberg™ works.

1.E.9. If you wish to charge a fee or distribute a Project Gutenberg™ electronic work or group of works on different terms than are set forth in this agreement, you must obtain permission in writing from the Project Gutenberg Literary Archive Foundation, the manager of the Project Gutenberg™ trademark. Contact the Foundation as set forth in Section 3 below.
1.F.
1.F.1. Project Gutenberg volunteers and employees expend considerable effort to identify, do copyright research on, transcribe and proofread works not protected by U.S. copyright law in creating the Project Gutenberg™ collection. Despite these efforts, Project Gutenberg™ electronic works, and the medium on which they may be stored, may contain “Defects,” such as, but not limited to, incomplete, inaccurate or corrupt data, transcription errors, a copyright or other intellectual property infringement, a defective or damaged disk or other medium, a computer virus, or computer codes that damage or cannot be read by your equipment.
1.F.2. LIMITED WARRANTY, DISCLAIMER OF DAMAGES - Except for the “Right of Replacement or Refund” described in paragraph 1.F.3, the Project Gutenberg Literary Archive Foundation, the owner of the Project Gutenberg™ trademark, and any other party distributing a Project Gutenberg™ electronic work under this agreement, disclaim all liability to you for damages, costs and expenses, including legal fees. YOU AGREE THAT YOU HAVE NO REMEDIES FOR NEGLIGENCE, STRICT LIABILITY, BREACH OF WARRANTY OR BREACH OF CONTRACT EXCEPT THOSE PROVIDED IN PARAGRAPH 1.F.3. YOU AGREE THAT THE FOUNDATION, THE TRADEMARK OWNER, AND ANY DISTRIBUTOR UNDER THIS AGREEMENT WILL NOT BE LIABLE TO YOU FOR ACTUAL, DIRECT, INDIRECT, CONSEQUENTIAL, PUNITIVE OR INCIDENTAL DAMAGES EVEN IF YOU GIVE NOTICE OF THE POSSIBILITY OF SUCH DAMAGE.
1.F.3. LIMITED RIGHT OF REPLACEMENT OR REFUND - If you discover a defect in this electronic work within 90 days of receiving it, you can receive a refund of the money (if any) you paid for it by sending a written explanation to the person you received the work from. If you received the work on a physical medium, you must return the medium with your written explanation. The person or entity that provided you with the defective work may elect to provide a replacement copy in lieu of a refund. If you received the work electronically, the person or entity providing it to you may choose to give you a second opportunity to receive the work electronically in lieu of a refund. If the second copy is also defective, you may demand a refund in writing without further opportunities to fix the problem.
1.F.4. Except for the limited right of replacement or refund set forth in paragraph 1.F.3, this work is provided to you ‘AS-IS’, WITH NO OTHER WARRANTIES OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO WARRANTIES OF MERCHANTABILITY OR FITNESS FOR ANY PURPOSE.
1.F.5. Some states do not allow disclaimers of certain implied warranties or the exclusion or limitation of certain types of damages. If any disclaimer or limitation set forth in this agreement violates the law of the state applicable to this agreement, the agreement shall be interpreted to make the maximum disclaimer or limitation permitted by the applicable state law. The invalidity or unenforceability of any provision of this agreement shall not void the remaining provisions.
1.F.6. INDEMNITY - You agree to indemnify and hold the Foundation, the trademark owner, any agent or employee of the Foundation, anyone providing copies of Project Gutenberg™ electronic works in accordance with this agreement, and any volunteers associated with the production, promotion and distribution of Project Gutenberg™ electronic works, harmless from all liability, costs and expenses, including legal fees, that arise directly or indirectly from any of the following which you do or cause to occur: (a) distribution of this or any Project Gutenberg™ work, (b) alteration, modification, or additions or deletions to any Project Gutenberg™ work, and (c) any Defect you cause.
Section 2. Information about the Mission of Project Gutenberg™
Project Gutenberg™ is synonymous with the free distribution of electronic works in formats readable by the widest variety of computers including obsolete, old, middle-aged and new computers. It exists because of the efforts of hundreds of volunteers and donations from people in all walks of life.
Volunteers and financial support to provide volunteers with the assistance they need are critical to reaching Project Gutenberg™’s goals and ensuring that the Project Gutenberg™ collection will remain freely available for generations to come. In 2001, the Project Gutenberg Literary Archive Foundation was created to provide a secure and permanent future for Project Gutenberg™ and future generations. To learn more about the Project Gutenberg Literary Archive Foundation and how your efforts and donations can help, see Sections 3 and 4 and the Foundation information page at www.gutenberg.org.
Section 3. Information about the Project Gutenberg Literary Archive Foundation
The Project Gutenberg Literary Archive Foundation is a non-profit 501(c)(3) educational corporation organized under the laws of the state of Mississippi and granted tax exempt status by the Internal Revenue Service. The Foundation’s EIN or federal tax identification number is 64-6221541. Contributions to the Project Gutenberg Literary Archive Foundation are tax deductible to the full extent permitted by U.S. federal laws and your state’s laws.
The Foundation’s business office is located at 809 North 1500 West, Salt Lake City, UT 84116, (801) 596-1887. Email contact links and up to date contact information can be found at the Foundation’s website and official page at www.gutenberg.org/contact
Section 4. Information about Donations to the Project Gutenberg Literary Archive Foundation
Project Gutenberg™ depends upon and cannot survive without widespread public support and donations to carry out its mission of increasing the number of public domain and licensed works that can be freely distributed in machine-readable form accessible by the widest array of equipment including outdated equipment. Many small donations ($1 to $5,000) are particularly important to maintaining tax exempt status with the IRS.
The Foundation is committed to complying with the laws regulating charities and charitable donations in all 50 states of the United States. Compliance requirements are not uniform and it takes a considerable effort, much paperwork and many fees to meet and keep up with these requirements. We do not solicit donations in locations where we have not received written confirmation of compliance. To SEND DONATIONS or determine the status of compliance for any particular state visit www.gutenberg.org/donate.
While we cannot and do not solicit contributions from states where we have not met the solicitation requirements, we know of no prohibition against accepting unsolicited donations from donors in such states who approach us with offers to donate.
International donations are gratefully accepted, but we cannot make any statements concerning tax treatment of donations received from outside the United States. U.S. laws alone swamp our small staff.
Please check the Project Gutenberg web pages for current donation methods and addresses. Donations are accepted in a number of other ways including checks, online payments and credit card donations. To donate, please visit: www.gutenberg.org/donate.
Section 5. General Information About Project Gutenberg™ electronic works
Professor Michael S. Hart was the originator of the Project Gutenberg™ concept of a library of electronic works that could be freely shared with anyone. For forty years, he produced and distributed Project Gutenberg™ eBooks with only a loose network of volunteer support.
Project Gutenberg™ eBooks are often created from several printed editions, all of which are confirmed as not protected by copyright in the U.S. unless a copyright notice is included. Thus, we do not necessarily keep eBooks in compliance with any particular paper edition.
Most people start at our website which has the main PG search facility: www.gutenberg.org.
This website includes information about Project Gutenberg™, including how to make donations to the Project Gutenberg Literary Archive Foundation, how to help produce our new eBooks, and how to subscribe to our email newsletter to hear about new eBooks.